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LINEAR HIGH BAY
ST36 SERIES







DESCRIPTION:
•  High luminous efficacy 140lm/w;
•  High quality non-isolated driver; 1-10V dimming; Flicker.
•  PF >0.90, driver efficiency >87%; THD<20%
•  LED Linear high bay lighting is a popular choice in warehouse lighting.
•  They are easy to hang with two gribber cables and easy to connect with the junction box right on
    back.
•  Popular for their wide light distribution, they are a great choice for going LED and saving energy.


APPLICATIONS:
•  Designed for warehouses, gymnasiums, and industrial spaces;


SPECIFICATIONS
	SKU
	Model
	[bookmark: OLE_LINK3]Wattage
	Size
	CCT
	Efficacy
	Lumens
	Input Current

	25-31170-xx
	ST36-LHB-12-7110-8XX-B
	110W
	1x2'
	4000K
	140 LPW
	15400 lm
	Max. 1.10A

	
	
	
	
	5000K
	
	
	

	25-31171-xx
	ST36-LHB-12-7165-8XX-B
	165W
	
	4000K
	
	23100 lm
	Max. 1.65A

	
	
	
	
	5000K
	
	
	

	25-31203-xx
	ST36-LHB-14-7225-8XX-B
	225W
	
	4000K
	
	31500 lm
	Max. 2.25A

	
	
	
	
	5000K
	
	
	

	25-31172-xx
	ST36-LHB-14-7225-8XX-B
	225W
	1x4'
	4000K
	
	31500 lm
	Max. 2.25A

	
	
	
	
	5000K
	
	
	

	25-31173-xx
	ST36-LHB-14-7320-8XX-B
	320W
	
	4000K
	
	44800 lm
	Max. 3.20A

	
	
	
	
	5000K
	
	
	



	Photomeritc

	CRI
	SDCM
	R9
	Duv
	Beam Angle

	≥80
	≤4
	≥0
	≤0.006
	90°



	Electrical

	Frequency
	Voltage
	Power Factor

	50/60Hz
	AC 120-277V
	≥0.90



	Lifetime [at 120-227V]

	[bookmark: OLE_LINK1]L70 Lumen Maintenance Life [Hour]
	L90 Lumen Maintenance Life [Hour]
	Warranty [Years]

	≥50000
	≥36000
	5








	Technical Requirements

	Certifications
	[bookmark: OLE_LINK5]UL I CE I FCC I RoHS

	THD
	≤20%

	Ripple Current
	≤5%

	Frequency of LED Current
	≥120Hz

	Flicker
	Flicker

	Electrostatic Discharge [ESD]
	4KV Contact discharge / 8KV Air discharge

	Surge Protection
	4KV

	Dimming
	1-10V

	Sensor
	Optional

	Emergency Power
	Optional

	IP Degree
	IP20



	Operation and Information

	Start Time
	≤1 S

	Operating Temp.
	-4℉~+113℉

	Storage Temp.
	-22℉~+149℉

	Housing / Case [Color, Material]
	White, Steel

	Optical - Lens [Material]
	PC

	Mounting / Installation
	[bookmark: OLE_LINK15]Pendant Mount / Surface Mount

	Environment
	Indoor / Suitable for damp location


[bookmark: OLE_LINK4]





LAMP CODE DEFINITIONS
	Internal Use
	Product Code
	Size
	Wattage
	CCT
	Version

	ST36
	LHB
	[bookmark: OLE_LINK7]12 = 1x2'
	110W
	8XX = 4000K,
4500K,
5000K,
5700K
	B

	
	
	
	165W
	
	

	
	
	
	225W
	
	

	
	
	14 = 1x4'
	225W
	
	

	
	
	
	320W
	
	





DIMENSIONS

1x2' 110W
[image: ST36-SIZE]












1x2' 165W
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1x2' 225W
[image: D:\EST-Rano\产品资料\Linear High Bay\ST59\尺寸图\2X2 220W灯体尺寸图.png2X2 220W灯体尺寸图]
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1x4' 225W
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1x4' 320W
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	[bookmark: OLE_LINK13]Product Size
	Wattage
	Long (L)
	Wide (W)
	High (H)
	Net Weight

	1x2'
	110W
	23.82''
	12.60''
	[bookmark: OLE_LINK12]2.99''
	10.14 lbs

	
	165W
	23.82''
	17.32''
	2.99''
	13.23 lbs

	
	225W
	23.64’’
	14.17’’
	2.89’’
	17.22lbs

	1x4'
	225W
	45.87''
	12.60''
	2.99''
	7.22 lbs

	
	320W
	45.87''
	17.32''
	2.99''
	22.49 lbs


[bookmark: OLE_LINK8]
PACKAGE
	Product Size
	Wattage
	Pcs / Carton
	Master Carton Size
	Gross Weight
	Pcs / Pallet

	[bookmark: OLE_LINK11][bookmark: OLE_LINK9]1x2'
	110W
	2 pcs
	[bookmark: OLE_LINK6]25.78'' x 8.66'' x 15.75''
	24.25 lbs
	80 pcs

	
	165W
	2 pcs
	[bookmark: OLE_LINK10]25.78'' x 8.66'' x 20.47''
	31.42 lbs
	64 pcs

	
	225W
	2 pcs
	
	
	

	1x4'
	225W
	2 pcs
	47.83'' x 8.66'' x 15.75''
	40.12 lbs
	40 pcs

	
	320W
	2 pcs
	47.83'' x 8.66'' x 20.47''
	49.38 lbs
	32 pcs



*Package specifications are subject to change without notic

CONTAINER LOADING
[image: 柜子][image: 柜子]




20GP Container                                                  40GP Container
	110w
	880pcs (No Pallet) | 640pcs (Palletized)
	
	110w
	1980pcs (No Pallet) | 1440pcs (Palletized)

	165w
	704pcs (No Pallet) | 512pcs (Palletized)
	
	165w
	1584pcs (No Pallet) | 1152pcs (Palletized)

	1’x2’
225w
	840pcs (No Pallet) | 480pcs (Palletized)
	
	1’x2’
225w
	750pcs (No Pallet) | 1080pcs (Palletized)

	1’x4’
225w
	460pcs (No Pallet) | 320pcs (Palletized)
	
	1’x4’
225w
	1010pcs (No Pallet) | 720pcs (Palletized)

	320w
	368pcs (No Pallet) | 256pcs (Palletized)
	
	320w
	808pcs (No Pallet) | 576pcs (Palletized)
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40HQ Container                                                  45HQ Container
	110w
	2340pcs (No Pallet) | 1440pcs (Palletized)
	
	110w
	2600pcs (No Pallet) | 1600pcs (Palletized)

	165w
	1800pcs (No Pallet) | 1152pcs (Palletized)
	
	165w
	2000pcs (No Pallet) | 1280pcs (Palletized)

	1’x2’
225w
	2100pcs (No Pallet) | 480pcs (Palletized)
	
	1’x2’
225w
	[bookmark: _GoBack]2400pcs (No Pallet) | 1200pcs (Palletized)

	1’x4’
225w
	1170pcs (No Pallet) | 720pcs (Palletized)
	
	1’x4’
225w
	1430pcs (No Pallet) | 800pcs (Palletized)

	320w
	900pcs (No Pallet) | 576pcs (Palletized)
	
	320w
	1100pcs (No Pallet) | 640pcs (Palletized)



AVAILABLE OPTIONS
	SKU
	Description
	Image

	[bookmark: OLE_LINK14]39-93011-A
	PIR Sensor Use for Low Altitude
	[image: 1][image: 红外无支架]

	39-93013-A
	PIR Sensor Use for High Altitude
	

	39-93017-A
	Microwave Sensor Use for Low Altitude
	[image: 39_看图王]

	39-93019-A
	Microwave Sensor Use for High Altitude
	

	37-31175-A
	Surface Mount
	[image: Surface Mount]

	37-31176-A
	Wire guard use 110W
	[image: 110w]

	37-31177-A
	Wire guard use 165W
	[image: 165w 220w]

	37-31178-A
	Wire guard use 225W
	[image: 215w]

	37-31179-A
	Wire guard use 320W
	[image: 320w]

	78-20178-A
	Remote Control with Standby Functions and Digital Display
	[image: 1][image: 1]

	44-33005-A
	Remote Control with Standby Functions
	[image: 1][image: D:\桌面\GLL产品图片\Backlit Panel LH18LH28\44-33005-A.png44-33005-A]

	44-33008-A
	Remote control On/Off Only
	[image: D:\桌面\GLL产品图片\Backlit Panel LH18LH28\44-33008-A.png44-33008-A]

	58-92057
	Emergency Power 15w, for 110w/165w LHB
	[image: C:\Users\Administrator\OneDrive\GLL-Rano\ZOHO ITEMS 图片\EBB single flex.pngEBB single flex]

	58-92058
	Emergency Power 20w, for 225w LHB
	

	58-92059
	Emergency Power 25w, for 320w LHB
	


	
Add: 79 Emjay Blvd. Brentwood New York USA 11717 | Tel: 516-218-5599 | E-mail: Service@builderspack.com | Web: www.builderspack.com
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