FEATURES               	
· 22 Gauge metal housing with matt white paint
· [image: de964b32f6097f249cfe832cb9e24e8]Smooth PMMA cover lens
· High efficacy meets premium;
· Lens & LED board build-in-one design
· Suspension and surface mount option
· Wattage & CCT selectable
· 5 Year warranty
· DC 12V Auxiliary
Applications                 
· Parking lot
· Supermarket
· Corridor
· Retail spaces
· Warehouses
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描述已自动生成] MLSN SERIES LED STRIPLIGHT(MULTI WATTAGE&CCT)

SHANGHAI HONGBAO LIGHTING CO.,LTD
NO.888, East HuiWang Road, JiaDing District, ShangHaI TEL: +86 21 31275320 FAX: +86 21 31272277
Ordering Information
	Name
	Length
	Wattage
	Dimming
	Driver
	CCT
	Backup
	Sensor

	MLSN
	2:2FT
	22
Or
20/24/28
	/D10:0-10V
	/U:120-277V
/W: 120-347
	35-40-50
	Blank: None
	Blank: None

	
	4:4FT
	22/28/36/44
	
	
	
	 Battery Backup
	    Sensor

	
	8:8FT
	44/58/68
	
	
	
	
	

	
	8:8FT
	48/68/90
	
	
	
	
	


Example:  MLSN4-22/28/36/44/D10/U/35-40-50/MS
( covers 22/28/36/44W 4FT 120-277V multi-CCT with motion sensor)

specifications
	Model
	MLSN2
	MLSN4
	MLSN8

	Wattage
	( Cover 22W)
(Cover 20/24/28)
	(covers22/28/36/44W)
	(Covers 44/58/68W)
(Covers48/68/90W)

	Voltage
	120-277V
120-347V

	LM/W 
	>130 @4000K

	CCT
	3500K-4000K-5000K

	CRI
	>80

	L70/L90
	100,000/40,000h

	Beam Angle
	120°

	Dimension(mm)
	610x68.8x65.5
	1183.6x68.8x65.5
	2357.6x68.8x65.5


Note: Actual performance may differ as a result of end-user environment and application. 
       All values are design or typical values, measured under laboratory conditions at 25 °C.  
Specifications subject to change without notice
photometric data
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	V-Hook
	Aircraft cable
	Chain
	Joiner bracket
	Backup pack
	Motion Sensor
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Accessories
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